**Terms of Reference**

**for the purchase of an electro-hydraulic press for Maintenance Department, Kumtor Gold Company CJSC**

|  |  |  |
| --- | --- | --- |
| Item № | Requirement parameters for the Goods to be purchased | Specific requirements for the Goods |
| 1 | Description and quantity | 40-ton electro-hydraulic press: 1 unit. |
| 2 | Delivery location | 9 Naryn highway, Balykchy, Kyrgyz Republic. |
| 3 | Delivery Deadline | To be specified in the Agreement. The shortest delivery period will be an advantage. |
| 4 | Requirements for the Goods to be supplied | 1. The supplied press shall be new, unused, certified or declared, fully compliant with quality standards, certificate of conformity, manufacturer's data sheet or technical specification. The press shall not be pledged, arrested, and shall be free from the rights of third parties. 2. The supplied press shall be produced in compliance with the requirements of regulatory documents (standards, technical specifications, quality certificates approved in accordance with the established procedure for this type of goods, etc.) under the serial production conditions. 3. The supplied press shall comply with the functional, technical and qualitative characteristics (operational characteristics) of the purchase object specified in this section. 4. The electro-hydraulic press shall comply with the environmental requirements established by the applicable laws of the Kyrgyz Republic. 5. The electro-hydraulic press shall comply with the safety requirements established by the applicable laws of the Kyrgyz Republic/EAEU. 6. The supplied electro-hydraulic press shall be new and unused. The press will be operated in high altitude conditions above 4,000 m above sea level, with the temperature range from - 40℃ to +40℃.   7. The electro-hydraulic press shall meet or exceed the requirements of the technical specifications in terms of performance and energy efficiency.  8. The press shall comply with the applicable safety requirements established by law.  9. The supplied press shall not be pledged, under arrest or another encumbrance.  10. Technical specifications of the 40-ton electro-hydraulic press:   * 1. Maximum force: 40 tons.   2. Maximum piston stroke: 200 mm.   3. Table lift height: 950 mm.   4. Maximum pump pressure: 20 MPa.   5. Electric motor power: 2.5–3 kW.   6. Power supply: 220/380 V, 50 Hz.   7. Dimensions (L\*W\*H): 1,300\*650\*1,850 mm. |
| 5 | Delivery and acceptance procedure | 1. When supplying the electro-hydraulic press, the Supplier shall provide: originals or duly certified copies of valid certificates of conformity and declarations of conformity to the requirements of regulatory documents for the supplied goods in the territory of the Kyrgyz Republic/EAEU.  2. After commissioning during the warranty period, the electro-hydraulic press shall be evaluated. The characteristics shall comply with the manufacturer's specifications.  3. In the event of non-compliance with the requirements, the Supplier shall bear all costs for its elimination.  4. All costs for additional work identified during the equipment inspection shall be borne by the Supplier. |
| 6 | Requirements for the submission of technical and other documents to the Client. | 1. Upon delivery of the Goods, the Supplier shall submit to the Client the consignment notes, invoices, as well as other documents such as service book, equipment passport, documents confirming the manufacturer's/supplier's quality warranty, operating instruction (manual). 2. All required user manuals and technical documentation shall be included in the package and shall not be accepted in the form of copies. |
| 7 | Warranty obligations. | 1. The Supplier shall provide a warranty period for the purchased equipment in accordance with the manufacturer's terms and conditions. |