**Terms of Reference**

**for the purchase of a stationary closed-type sandblasting cabinet for Maintenance Department of Kumtor Gold Company CJSC**

|  |  |  |
| --- | --- | --- |
| Item № | Requirement parameters for the Goods to be purchased | Specific requirements for the Goods |
| 1 | Description and quantity | Stationary closed-type sandblasting cabinet (hereinafter referred to as the sandblasting cabinet): 1 unit. |
| 2 | Delivery location | 9 Naryn highway, Balykchy, Kyrgyz Republic. |
| 3 | Delivery Deadline | To be specified in the Agreement. The shortest delivery period will be an advantage. |
| 4 | Requirements for the Goods to be supplied | 1. The supplied cabinet shall be new, unused, certified or declared, fully compliant with quality standards, certificate of conformity, manufacturer's data sheet or technical specification. The cabinet shall not be pledged, arrested, and shall be free from the rights of third parties. 2. The supplied cabinet shall be produced in compliance with the requirements of regulatory documents (standards, technical specifications, quality certificates approved in accordance with the established procedure for this type of goods, etc.) under the serial production conditions. 3. The supplied cabinet shall comply with the functional, technical and qualitative characteristics (operational characteristics) of the purchase object specified in this section. 4. The sandblasting cabinet shall comply with the environmental requirements established by the applicable laws of the Kyrgyz Republic. 5. The sandblasting cabinet shall comply with safety requirements. 6. The supplied sandblasting cabinet shall be new and unused. The cabinet will be operated in high altitude conditions above 4,000 m above sea level, with the temperature range from - 40℃ to +40℃.   7. The sandblasting cabinet shall meet or exceed the requirements of the technical specifications in terms of performance and efficiency.  8. The cabinet shall comply with the applicable safety requirements established by law.  9. The supplied cabinet shall not be pledged, under arrest or another encumbrance.  10. Technical specifications of the sandblasting cabinet:   * 1. Operating chamber (W x L x H), mm: 1,250 x 1,250 x 2,150.   2. Pressure: ≈ 8 MPa.   3. Efficiency: ≈ 10 m²/h.   4. Air consumption: 3-7 m³/min.   5. Cleaning process: abrasive sand.   6. Lighting: built-in, dust protected.   7. Filtration system: built-in dust collector or connection to an external exhaust.   8. Gloves: built-in, wear-resistant, chemically resistant, with an additional spare pair.   9. Viewing window: impact-resistant glass with protective film. |
| 5 | Delivery and acceptance procedure | 1. When supplying the sandblasting cabinet, the Supplier shall provide: originals or duly certified copies of valid certificates of conformity and/or declarations of conformity to the requirements of regulatory documents.  2. After commissioning during the warranty period, the cabinet shall be evaluated. The characteristics shall comply with the manufacturer's specifications.  3. In the event of non-compliance with the requirements, the Supplier shall bear all costs for its elimination.  4. All costs for additional work identified during the cabinet inspection shall be borne by the Supplier.  5. Training on the sandblasting cabinet operation shall be provided. |
| 6 | Requirements for the submission of technical and other documents to the Client. | 1. Upon delivery of the Goods, the Supplier shall submit to the Client the consignment notes, invoices, as well as other documents such as service book, equipment passport, documents confirming the manufacturer's/supplier's quality warranty, operating instruction (manual). 2. All required user manuals and technical documentation shall be included in the package and shall not be accepted in the form of copies. |
| 7 | Warranty obligations. | 1. The Supplier shall provide a warranty period for the purchased equipment in accordance with the manufacturer's terms and conditions. |