**Terms of Reference**

**For the purchase of a 200-ton press for the Maintenance department of the “Kumtor Gold Company” CJSC**

|  |  |  |
| --- | --- | --- |
| # | Requirement parameters for the purchased Goods | Specific requirements for Goods |
| 1 | Name and quantity | Press, in the amount of 1 unit. |
| 2 | Place of delivery of Goods | Kyrgyz Republic, Balykchy town, Naryn Highway Street 9. |
| 3 | Time limits (periods) for delivery of Goods. | It shall be provided for in the contract. The shortest delivery time will be an advantage. |
| 4 | Requirements for the supplied Goods | 1. The proposed Goods must be new, unused, certified, or declared, fully compliant with quality standards, certificate of conformity, the Manufacturer’s technical passport, or technical specifications. The Goods must not be pledged, seized, and must be free from third-party rights. 2. The proposed Goods must be manufactured in compliance with regulatory requirements (standards, technical conditions, quality certificates approved in the prescribed manner for this type of goods, etc.) under conditions of serial production. 3. The proposed Goods must meet the functional, technical, and quality characteristics (operational characteristics) of the procurement object specified in this section. 4. The Press must comply with the environmental requirements established by the current legislation of the Kyrgyz Republic. 5. The Press must comply with the safety requirements established by the current legislation of the Kyrgyz Republic / EAEU. 6. The supplied Press must be new, never used. Application area: at altitudes above 4000 m above sea level, at temperatures from -40 °C to +40 °C. 7. The Press must meet or exceed the technical specifications for performance and energy efficiency indicators. 8. The Goods must comply with current safety requirements established by law. 9. The supplied Goods must not be pledged, under arrest, or subject to any encumbrance.   10. Technical Specifications of the Press:   * 1. Maximum load 2000 kN.   2. The force is 200 tons.   3. Motor power: 4 kW, two-speed.   4. Operating voltage 380 V, 50 Hz (3-phase).   5. Nominal pressure 31.5 MPa.   6. Working table dimensions:   Table length – from 1600 to 1700 mm.  Distance between table and slider: when the table is installed on the upper slot – from 400 to 500 mm, when installed on the lower slot – from 1300 to 1400 mm.   * 1. Working table height adjustment by winch.   2. Control: semi-automatic (hydraulic drive with push-button control, pressure gauge, emergency stop). |
| 5 | Procedure for delivery and acceptance of Goods. | 1. When delivering the press, the Supplier must provide originals or duly certified copies of valid certificates of conformity and declarations of compliance with regulatory requirements for the supplied goods within the territory of the Kyrgyz Republic / EAEU.  2. After commissioning, during the warranty period, the press will be evaluated. Its characteristics must correspond to the manufacturer’s specifications.  3. In case any discrepancies with our requirements are identified, the Supplier shall bear all costs for their elimination.  4. All costs for additional work identified during equipment inspection shall be borne by the Supplier.  5. Conduct training on the operation of the Press. |
| 6 | Requirements for providing technical and other documentation to the Customer | 1. Upon delivery of the goods, the Supplier must provide the Customer with a waybill, invoice, and other documents: service book, equipment passport, documents confirming the provision of quality guarantees by the Manufacturer and the Supplier, and an operation manual (user guide). 2. All necessary user manuals and technical documentation must be included in the package and must not be provided as copies. |
| 7 | Warranty obligations | 1. The Supplier must provide a warranty period for the purchased equipment in accordance with the Manufacturer’s terms. |