**Terms of Reference**

**for the purchase of a jack for the Bendpak hoist for the Maintenance department of the Kumtor Gold Company CJSC**

|  |  |  |
| --- | --- | --- |
| Item # | Requirements parameters of the purchased Goods | Specific requirements for Goods |
| 1 | Name and quantity | Bendpak RBJ15000 jack or equivalent for a four-post lift, quantity – 1 unit |
| 2 | Place for Goods delivery | Kyrgyz Republic, Balykchy town, 9 Naryn Highway St. |
| 3 | Terms (periods) for Goods delivery | Provide for in the contract. The shortest delivery time will be an advantage. |
| 4 | Requirements for the supplied Goods | 1. The proposed Goods must be new, unused, certified, or declared, and fully compliant with quality standards, the certificate of conformity, the manufacturer’s technical passport, or the manufacturer’s technical specification. The Goods must not be pledged, seized, and must be free of any third‑party rights. 2. The proposed Goods must be manufactured in compliance with the requirements of regulatory documents (standards, technical specifications, quality certificates approved in the prescribed manner for this type of goods, etc.) under conditions of serial production. 3. The proposed Goods shall comply with the functional, technical, and quality characteristics (operational characteristics) of the procurement object specified in this Section. 4. The Goods comply with the safety requirements established by the current legislation of the Kyrgyz Republic / EAEU. 5. The supplied jack must be new and not previously used. It must be suitable for operation at altitudes above 4,000 meters above sea level and at temperatures from –40 °C to +40 °C.   6. The jack must meet or exceed the requirements of technical specifications for performance and energy economic indicators.  7. The Goods must comply with the current safety requirements established by applicable legislation.  8. The supplied Goods must not be pledged, arrested, or otherwise encumbered.  9. Technical specifications for the Bendpak RBJ15000 Lift Jack:   * + Lifting capacity: 15,000 lbs (≈ 6,804 kg)   + Rolling Bridge Jack   + Suitable for BendPak HDS‑27 four‑post lift   + Minimum lifting height: with short lift pad: 14" (356 mm), with adapter: 17" (432 mm)   + Maximum lifting height: with short lift pad: 23" (584 mm), with adapter: 26" (660 mm)   + Support base width: from 44.9" to 63.75" (≈ 1,140 - 1,619 mm)   + Drive type: pneumohydraulic.   + Accessories: stackable height‑extension adapters and   telescoping arms for width adjustment for various wheelbases |
| 5 | Procedure for Goods delivery and acceptance | 1. Provision of original certificates of conformity or certified copies 2. Assessment of compliance of characteristics after commissioning 3. In case of non-conformities, elimination is at the expense of the Supplier |
| 6 | Requirements for the transfer of technical and other documents for the Goods to the Customer | 1. Bill of lading, invoice, equipment passport, operating manual, warranty documents 2. All documentation must be original; copies are not permitted |
| 7 | Warranty obligations | 1. The Supplier must provide a warranty period for the purchased equipment in accordance with the Manufacturer’s warranty conditions. |