**Техническое задание**

**на поставку фронтального погрузчика для Подземной разработки ЗАО «Кумтор Голд Компани»**

|  |  |  |
| --- | --- | --- |
| **№**  **п/п** | **Перечень основных**  **данных и требований** | **Основные данные и требования** |
| 1. | Место доставки | ЗАО «КУМТОР ГОЛД КОМПАНИ». Кыргызская Республика, г. Балыкчы, ул. Нарынское шоссе, 9. |
| 2. | Заказчик | ЗАО «Кумтор Голд Компани», Подземная разработка |
| 3. | Общие положения | Предметом настоящего технического задания является приобретение двух единиц фронтального погрузчика, предназначенных для погрузки, перемещения и складирования инертных материалов (щебень, песок, грунт) на поверхности. Оборудование должно быть новым, не бывшим в эксплуатации и не восстановленным |
| 4. | Условия эксплуатации | Высота над уровнем моря — до 4000 м.; температура окружающего воздуха от −35 °C до +40 °C.  Дорожные условия: карьерные и технологические дороги с уклонами до 15 %, покрытие — щебень/грунт/порода. |
| 5. | **Требования к оборудованию** |  |
| 5.1. | Требования к шасси | Колесная формула 4×4 |
| 5.2. | Двигатель | Тип: Дизельный двигатель с турбонаддувом, арктический пакет.  Система охлаждения жидкостная; предпусковой подогрев; |
| 5.3. | Ковш | Объем ковша – 3–4 м³ (универсальный, с кромкой и защитой зубьев). |
| 5.4. | Тормозная система | Рабочий тормоз – гидравлическая двухконтурная система, многодисковые тормоза в масляной ванне; Стояночный тормоз – обратного действия, пружинный, гидравлическое отключение. |
| 5.5. | Шины | Пневматические, бескамерные, типоразмер – по согласованию, запасное колесо – минимум 1 шт. |
| 5.6. | Электрооборудование | Бортовая сеть 24 В, рабочее освещение, проблесковый маячок; звуковая сигнализация заднего хода. |
| 5.7. | Кабина | Закрытая кабина, кондиционер и отопление, сиденье с пневмоподвеской, зеркала и камера заднего вида, мультимедийный/информационный дисплей с показателями: скорость, обороты, давление, температуры, коды ошибок. |
| 5.8. | Противопожарная система | Автоматическая система пожаротушения в двигательном отсеке, переносные огнетушители. |
| 5.9 | Гидравлическая система | Насосы с переменной производительностью, фильтрация масла, индикация уровня и температуры, быстросъемные соединения – по согласованию. |
| 6. | ЗИП и инструменты | Комплект ЗИП на 2 000 моточасов / 1 год эксплуатации: фильтры (двигатель/гидросистема), ремни, уплотнения,  запасные элементы гидросистемы. |
| 7. | Техническая документация | 1. Поставщик вместе с оборудованием обязуется предоставить сопроводительную техническую документацию (сертификаты соответствия, технические паспорта, инструкции по эксплуатации, каталог запасных частей и другие необходимые документы для безопасной эксплуатации, а также для прохождения таможенного оформления и регистрации в государственных органах КР). 2. Инструкции по эксплуатации и ТО. 3. Каталог на запасные части в бумажном переплете и в электронном виде. 4. Документация формате PDF. 5. Сертификат качества и происхождения,   *Все документы должны быть предоставлены как в электронном виде, так и в бумажном на русском и английском языках.* |
| 8. | Гарантийный срок | 1. Поставщик должен предоставить гарантийный срок на приобретаемое оборудование до 12 месяцев со дня ввода в эксплуатации, 2. Наличие сервис центра и склада запасных частей на территории КР. 3. В случае отсутствия сервисного центра и склада запасных частей на территории страны Заказчика. Поставщик обязуется создать необходимые условия для организации сервисного обслуживания и технической поддержки в стране пребывания Заказчика. |
| 9. | Приемка оборудования | Приемка оборудования по качественным и количественным показателям производится на месте доставки. |
| 10. | Запуск | 1. Все затраты за дополнительные работы выявленные в ходе проверки оборудования несет Поставщик. |
| 11. | Критерии оценки качества | 1. После ввода в эксплуатацию в течение гарантийного срока производится оценка оборудования. Характеристика должна соответствовать заводским показаниям. 2. В случае выявления несоответствий наших требований Поставщик берет на себя все затраты по их устранению. |
| 12. | Условия оплаты и сроки поставки | 1. Условия оплаты: согласно Договору. 2. Доставка осуществляется за счет и силами Поставщика. 3. Условия поставки: для нерезидентов КР- DAP, для резидентов КР -DDP. 4. Место доставки: Кыргызская Республика, г. Балыкчы, ул. Нарынское шоссе, 9. 5. Срок поставки: до 90 календарных дней с момента подписания Договора Сторонами. |
| 13. | Технические регламенты и стандарты | Оборудование должно соответствовать требованиям, установленным действующим Техническим регламентом Таможенного союза (ТР ТС 010/2011) «О безопасности машин и оборудования» и другими действующими требованиями ЕАЭС (при необходимости). |
| 14. | Безопасность | Системы блокировки торможения и защиты от перегрузов, противопожарные средства и освещение в соответствии с техническими паспортами.  Движущиеся части оборудования, представляющие собой источник опасности для людей, должны быть ограждены, за исключением частей, ограждение которых невозможно из-за их функционального назначения. Ограждения, должны поставляться комплектно с техническими устройствами для установки данного ограждения. |
| 15. | Примечание | Требования, указанные в настоящем ТЗ, является ориентировочным и может быть скорректировано в процессе обсуждения с потенциальными поставщиками. |

**Terms of Reference**

**for the supply of a front-end loader for Underground Mining Department, Kumtor Gold Company CJSC**

|  |  |  |
| --- | --- | --- |
| **Item**  **№** | **List of basic data and requirements** | **Basic data and requirements** |
| 1. | Delivery location | KUMTOR GOLD COMPANY CJSC, 9 Naryn highway, Balykchy, Kyrgyz Republic. |
| 2. | Client | Kumtor Gold Company CJSC, Underground Mining. |
| 3. | General provisions | The subject of these Terms of Reference is the purchase of 2 (two) units of front-end loaders designed for loading, transporting, and stockpiling inert materials (crushed stone, sand, soil) on the surface. The equipment shall be brand new, unused, and not refurbished. |
| 4. | Operating conditions | Altitude above sea level: up to 4,000 m. Ambient air temperature ranging from −35 °C to +40 °C.  Road conditions: pit roads and technological roads with slopes up to 15%. Surface: crushed stone/soil/rock. |
| 5. | **Requirements for the equipment** |  |
| 5.1. | Chassis requirements | Wheel configuration: 4×4. |
| 5.2. | Engine | Type: turbocharged diesel engine, Arctic package.  Cooling system: liquid cooled. Pre-start heating system. |
| 5.3. | Bucket | Bucket capacity: 3–4 m³ (universal, with cutting edge and tooth protection). |
| 5.4. | Braking system | Service brake: hydraulic dual-circuit system, multi-disc brakes in an oil bath. Parking brake: fail-safe spring-applied, hydraulic shutdown. |
| 5.5. | Tires | Pneumatic, tubeless, size to be agreed. Spare wheel: at least 1 pc. |
| 5.6. | Electrical equipment | 24 V on-board electrical system, work lighting, flashing light, reverse alarm. |
| 5.7. | Cab | Enclosed cab with air conditioning and heating, air-suspended seat, mirrors and rear-view camera, multimedia/information display showing speed, engine RPM, pressure, temperatures, and error codes. |
| 5.8. | Fire protection system | Automatic fire suppression system in the engine compartment, portable fire extinguishers. |
| 5.9 | Hydraulic system | Variable displacement pumps, oil filtration, level and temperature indicators, quick-release couplings: to be agreed. |
| 6. | Spare parts and tools | Spare parts kit for 2,000 operating hours/1 year of service:  filters (engine/hydraulic system), belts, seals,  spare hydraulic system components. |
| 7. | Technical documentation | 1. The Supplier shall provide, along with the equipment, all supporting technical documentation (certificates of conformity, technical passports, user manuals, spare parts catalogs, and any other documents required to ensure safe operation, facilitate customs clearance, and support registration with the relevant state authorities of the Kyrgyz Republic). 2. Operating and maintenance instructions. 3. Spare parts catalog in printed hardcover and electronic formats. 4. Documentation in PDF format. 5. Certificate of quality and origin.   *All documents shall be provided both in electronic and hard copy formats, in Russian and English.* |
| 8. | Warranty period | 1. The Supplier shall provide a warranty period for the purchased equipment of up to 12 months from the date of commissioning. 2. Service center and spare parts warehouse within the territory of the Kyrgyz Republic shall be available. 3. If service center and spare parts warehouse are not available within the Client’s country, the Supplier shall establish the necessary arrangements to ensure proper maintenance and technical support at the Client’s location. |
| 9. | Equipment acceptance | The equipment shall be accepted based on quality and quantity criteria at the delivery location. |
| 10. | Commissioning | 1. All costs for additional work identified during the equipment inspection shall be borne by the Supplier. |
| 11. | Quality evaluation criteria | 1. After commissioning, the equipment shall be evaluated during the warranty period. Evaluation results shall comply with the manufacturer's specifications. 2. In the event of non-compliance with KGC requirements, the Supplier shall bear all costs for its elimination. |
| 12. | Payment and delivery terms | 1. Payment terms: as specified in the Agreement. 2. The equipment shall be delivered at the Supplier’s expense and responsibility. 3. Delivery terms: for non-residents of the Kyrgyz Republic – DAP, for residents of the Kyrgyz Republic – DDP. 4. Delivery location: 9 Naryn highway, Balykchy, Kyrgyz Republic. 5. Delivery deadline: up to 90 calendar days from the date of signing the Agreement by the Parties. |
| 13. | Technical regulations and standards | The equipment shall comply with the requirements established by the applicable Technical Regulations of the Customs Union (TR CU 010/2011) “On the Safety of Machinery and Equipment” and other applicable EAEU requirements (if necessary). |
| 14. | Safety | Brake lock and overload protection systems, fire safety equipment, and lighting shall comply with the specifications outlined in the technical passports.  Moving parts of equipment that pose a hazard to people shall be guarded, except for those parts that cannot be guarded due to their functional purpose. Guards shall be provided as a complete set, including all necessary components and equipment for proper installation. |
| 15. | Note | The requirements set forth in these Terms of Reference are provisional and may be revised during negotiations with potential suppliers. |