
					
Terms of Reference for the Purchase of
Hydraulic Diaphragm Metering Pumps

	Item #
	Requirements parameters of for the goods, work, or services being purchased (subject of procurement)
	Specific requirements for the goods, work, or services

	1
	Name/type, quantity/volume, unit of measurement
	Hydraulic diaphragm metering pump – 8 units.

	2
	Place of delivery of goods or provision of services/performance of works
	Available delivery options:
A. Delivery to the Customer’s address:
9, Naryn Highway, Balykchy town, Issyk-Kul Region, Kyrgyz Republic.
B. Ex Works (EXW) collection from the manufacturer’s facility, with onward transportation arranged by the Customer.

	3
	Delivery period(s) for goods or period(s) for provision of services/performance of works
	· The equipment delivery period shall be specified by the Bidder in its commercial proposal.
· The proposed equipment delivery period will be considered together with the technical and commercial terms when evaluating bids.

	4
	Procedure (sequence and stages) for the supply and acceptance of the equipment
	1. The Supplier shall submit a commercial proposal in accordance with the tender documentation requirements.
2. The commercial proposal shall include all required technical and commercial documents, including the manufacturer’s quality certificates for the proposed equipment.
3. The Supplier shall properly prepare the equipment for transportation, including packaging, preservation, and marking sufficient to protect it during transit.
4. If selected as the successful Bidder, the Supplier shall deliver the equipment to the address specified by the Customer or dispatch it in accordance with the instructions of Kumtor Gold Company CJSC.
5. Upon arrival of the equipment at Kumtor Mine, specialists of Kumtor Gold Company CJSC will conduct an incoming inspection to verify compliance with the technical requirements, completeness, and absence of damage.
6. After installation and commissioning by the Customer, a signed Equipment Installation Certificate will be provided to the Supplier.

	5
	Requirements for the goods supplied, works performed, or services provided
	1. The equipment supplied shall be an industrial-grade hydraulic diaphragm metering pump designed for continuous heavy-duty operation 24 hours a day, 365 days a year, with shutdowns only for scheduled maintenance. The pump shall be suitable for pumping Sodium Amyl Xanthate (SAX) solution containing up to 25% solids, with a viscosity of 5–20 cP, at an operating pressure of up to 80 bar and at an installation elevation of 4,100 m above sea level.

	6
	Technical performance and design requirements
	1. The pump shall provide:
· a flow-rate range of 0.3 to 10 L/min.
· a nominal flow rate of 2.8 L/min.
· automatic capacity control by an external 4–20 mA analog signal.
· local and remote control.
· integration with the existing PLC/DCS system.
· continuous operation without degradation in performance.
2. The pump design shall include:
· hydraulic diaphragm actuation.
· a diaphragm integrity monitoring system (Diaphragm Rupture Detection).
· pressure overload protection.
· the ability to adjust capacity without stopping the equipment.
· wet-part materials of at least SS316L or equivalent corrosion resistance.

	7
	Requirements for transfer of technical and other documentation to the Customer upon completion and acceptance
	The Supplier shall provide:
· technical data sheet.
· operation and maintenance manual.
· manufacturer’s quality certificates.
· list of recommended spare parts for two years of operation.
· Factory Acceptance Test (FAT) reports, if available.

	8
	Warranty obligations
	The warranty period for the supplied equipment shall be at least 24 months from the date of commission or 30 months from the date of delivery, whichever occurs first.
During the warranty period, the Supplier shall:
· Remedy, free of charge, equipment defects attributable to the manufacturer or arising from the use of substandard materials.
· replace defective assemblies, parts, and components at their own expense, including the cost of spare parts and delivery.
· provide technical support to the Customer on equipment operation and maintenance.
· provide recommendations for troubleshooting and fault rectification.
· ensure delivery of warranty spare parts within agreed timeframes.
· in the event of a warranty failure, provide a report on the cause of failure and a list of corrective actions taken.
· guarantee the availability of service support and spare parts for the proposed equipment for at least 10 years after delivery.
Additionally:
· The warranty shall cover the complete pump assembly, drive, automatic capacity-control system, controllers, sensors, and other components included in the scope of supply.
· the initial response time to the Customer’s warranty claim shall not exceed 48 hours from receipt of the notification.
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