|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| # | Request items for CP | Quantity | Measure Unit | Planned unit price | Planned cost |
| 1 | Self-regulating heating cable, 230 V, 25 W/m at 10°C (8BTV2-CT) / CABLE, HEATING, SELF-REGULATING, 230V, 25 W/NAT 10°C | 200 | MT | 17,97 | 3594,00 |
| 2 | End Seal Kit, universal, cold-applied, installed under thermal insulation (E-150), ATEX / SEAL KIT, LOW PROFILE RAYCHEM END | 135 | EA | 120,49 | 16266,15 |
| 3 | Electronic Local Controller with Protective Temperature Limiter and Centralized Monitoring Capabilities (Elexant 5010i-LIM)/ UNIT, CONTROL, HEAT TRACING, ELECTRONIC LOCALCONTROL, CENTRAL MONITORING, WITH SAFETY TEMPERATURE LIMITER | 3 | EA | 1615,30 | 4845,90 |
| 4 | Remote Monitoring Module (RMM3)/ REMOTE MONITORING MODULE FOR UP TO 8 TEMPERATURE SENSORS, DIN-RAIL MOUNTABLE | 3 | EA | 1273,83 | 3821,49 |
| 5 | External Control Module for / DIGITRACE NGC-30 И MONITRACE 200N / MONI-RMC-BASE (309735–000) / EXTERNAL CONTROL MODULE FOR DIGITRACE NGC-30 AND MONITRACE 200N / MONI-RMC BASE | 3 | EA | 1883,79 | 5651,79 |
| 6 | User Interface Terminal for heat tracing system, enclosed for remote wall mounting (NGC-UIT3-ORD-R) / INTERFACE, USER INTERFACE TERMINAL IN ENCLOSURE FOR REMOTE MOUNTING ON WALL#OEM NGC-UIT2- ORD-R | 1 | EA | 8213,35 | 8213,35 |
| 7 | Cable Fault Locator Device / DIGITRACE OEM# DET-4000 IS A DEVICE FOR DETERMINING THE PLACES OF CABLE DAMAGE / SIDEKICK PLUS - HEAD HELD CABLE FAULT LOCATOR | 2 | EA | 6635,00 | 13270,00 |
| 8 | Heating cable (1244-020944) / CABLE, HEATING, SELF-REGULATING, 230V, 29 W/MAT 10°C, 10BTV2-CT | 230 | MT | 19,25 | 4427,50 |
| 9 | Temperature sensor with cable (with M16 gland M16) / SENSOR, TEMPERATURE WITH MI CABLE (WITH M16 GLAND) | 2 |  | 212.18 | 424.36 |