

**TERMS OF REFERENCE**

for the purchase of 4x4 off-road vehicles for the mine site of Kumtor Gold Company CJSC

|  |  |  |
| --- | --- | --- |
| **Item****№** | **List of basic** **data and requirements** | **Basic data and requirements** |
| 1. | Location  | Issyk-Kul Region, Jeti-Oguz District, Kumtor Gold Deposit. |
| 2. | Client  | Kumtor Gold Company CJSC. |
| 3. | Purpose of the purchase | The subject of the Terms of Reference is the purchase of 20 units of Toyota Land Cruiser 4.2 MT Double Cabin  |
| 4. | General requirements/Regulations and standards | 1. The delivered vehicle (hereinafter referred to as the vehicle) shall be new, not used.

Type - jeep, passenger car, belonging to category B vehicles. Purpose - driving on public roads, for transportation of people.Scope of operation - on highways, ground and mountain roads at an altitude of over 4,000 m above sea level, at temperatures from -35°C to +40°C.1. The vehicle shall meet or exceed the performance and energy efficiency requirements of the technical specifications.
2. All necessary user manuals and technical documentation shall be included, not as copies.
3. The vehicle shall comply with the applicable safety requirements established by law.
4. When delivering the vehicle, the Supplier shall submit: originals or duly certified copies of valid certificates of conformity and declarations of conformity to the requirements of regulatory documents for the goods delivered in the territory of the Kyrgyz Republic/EAEU.
5. The delivered vehicle shall not be pledged, under arrest or under any other encumbrance.
 |
| 5. | Technical specifications | * 1. Accessories: basic.
	2. Mileage: not more than 20 km.
	3. Tank volume: from 130 liters.
	4. Model: Land Cruiser 79 Double Cabin
	5. Type: cargo-passenger.
	6. Year of manufacture: 2024 and later.
	7. Overall dimensions (L x W x H): 5220 x 1690 x 1955.
	8. Number of seats: 5.

2. Engine2.1 Brand: 1HZ.2.2 Fuel: Diesel. 2.3 Volume: 4,163 cc.2.4 Power: from 130 hp and higher.2.5 Availability of turbine: With possibility of installation.3. Transmission gearbox3.1 Type: mechanical.3.2 Number of gears: 5.4. Axes 4.1 Wheel arrangement: 4х4.4.2 Wheel size: 245/65 R16.4.3 Tire type: tubeless MT.5. Additional information5.1 Color: White (preferred).5.2 Active and passive safety systems. 5.3 Antilock Braking System (ABS).5.4 Air conditioner. 5.5 Adaptation to operation in high altitude and cold climate. |
| 6. | Payment and delivery terms | Payment terms: to be agreed with the Client.The vehicle shall be delivered by the manufacturer to Bishkek or BMY within the deadlines specified by the Client.The vehicle shall be assembled and commissioned within the deadlines specified by the Client.In case of failure to comply with the terms, penalties shall apply. |
| 7. | Acceptance | 1. The vehicle shall be accepted on the Client's premises in the Supplier's presence.
2. All costs for additional work identified during the equipment inspection shall be borne by the Supplier.
 |
| 8. | Warranty period  | 1. The Supplier shall provide a warranty period for the purchased equipment in accordance with the manufacturer's terms and conditions.
 |
| 9. | Training and operation manual | 1. Operation manual for the vehicle shall be included.
 |
| 10. | Quality evaluation criteria | 1. After commissioning, the vehicle shall be evaluated during the warranty period and shall comply with the manufacturer's specifications.
2. In case of non-compliance with KGC requirements, Supplier shall assume all costs for its elimination.
3. The vehicle shall comply with the safety requirements established by the applicable laws of the Kyrgyz Republic/EAEU.
 |
| 11. | Confidentiality | 1. The transaction data shall be confidential. Disclosure to third parties shall be prohibited.
 |