Kumtor Gold Company CJSC invites to submit price proposals for the repair/replacement and maintenance of the Brand Kitchen Safe kitchen fire suppression equipment installed under the exhaust hoods of the canteen at the camp of Kumtor Gold Company CJSC
	Submission format:
	The application and other documents must be signed by a person authorized to sign the application and contractual obligations. Documents must be stamped with the company seal and submitted in PDF format. The signatory’s authority must be confirmed by a power of attorney or certified copies of the relevant documents.

	Proposal submission procedure
	Bidding participants must submit their proposal in Russian in accordance with the tender requirements, attach the necessary copies of documents and send them electronically to Zhyldyzkan.satybekova@kumtor.kg by 17:00 (Bishkek time) on 27 November 2026.
Bids received later or sent to any other e-mail address will not be considered.

	The application must contain the following documents:
	A commercial proposal specifying
∙ Service delivery timeframes
∙ Payment terms 
∙ Validity period of the commercial proposal (at least 40 calendar days)


	Evaluation criteria:
	The proposal offering the lowest price and optimal timeframes will be declared the winner of the tender.

	Send the commercial proposal to Zhyldyzkan.satybekova@kumtor.kg by 17:00 (Bishkek time) on 27 November 2026.


	The Customer reserves the right to accept or reject any or all proposals, and to cancel the tender process at any time prior to the award of the Contract, without thereby incurring any liability to the affected participants. 

	The commercial proposal must be submitted on official letterhead.
Residents must submit the commercial proposal in the national currency, without reference to a foreign currency exchange rate.

Non-residents may submit the commercial proposal in any currency.


	Bid proposals submitted by bidders after the specified deadline will not be accepted or considered.

Each bidder may submit only one tender proposal.

The bid proposal must remain valid for at least 40 calendar days.
No changes to bid proposals are permitted during the proposal validity period. 

	All questions regarding this bidding must be sent by e-mail to Zhyldyzkan.satybekova@kumtor.kg 

Requests for clarification of the bidding conditions must be submitted no later than 3 calendar days before the proposal submission deadline.








TERMS OF REFERENCE
for the repair/replacement and maintenance of the Brand Kitchen Safe kitchen fire suppression equipment installed under the exhaust hoods of the canteen at the camp of Kumtor Gold Company CJSC
	№
	List of key 
data and requirements
	Key data and requirements

	1
	Item name
	
Brand Kitchen Safe kitchen fire suppression system

[image: БКС кухонное пожаротушение]	

	2
	Site location
	Issyk-Kul Region, Djeti-Oguz District, Kumtor gold mine

	3
	Customer
	Kumtor Gold Company CJSC

	4
	Contractor 
	To be determined based on the selection results

	5
	Grounds for the works
	The need to restore and ensure the proper technical condition and continued safe operation of the Brand Kitchen Safe automatic kitchen fire suppression system in accordance with the requirements of applicable fire safety regulations and the manufacturer’s operating documentation, or, alternatively, its complete replacement taking into account the equipment’s service life.

	6
	Subject of the Terms of Reference 
	These Terms of Reference set out the requirements for performing a set of works comprising:
· Diagnostics of the system’s technical condition:
· Repair of faulty components;
· Maintenance;
· Functional testing;
· Adjustment and commissioning of the Brand Kitchen Safe automatic kitchen fire suppression system installed under the exhaust hoods of the canteen’s process equipment;
· If necessary, complete replacement of the equipment, taking into account its service life. 

	7
	Purpose of the system 
	The Brand Kitchen Safe system is designed for the automatic detection and containment of fires in cooking areas.

	8
	Objectives of the works
	The objectives of the works are:
· To restore full functionality of the system;
· To ensure reliable fire protection of kitchen equipment and premises;
· To ensure compliance of the system with fire safety requirements;
· To prevent emergencies and the risk of fire spreading;
· To ensure proper operation of the system’s automatic and manual activation.
· If necessary, complete replacement of the equipment, taking into account its service life. 

	9
	Repair works
	Based on the diagnostic results, the Contractor shall repair and replace faulty components, including but not limited to:
· Replacement of nozzles;
· Replacement of fusible links;
· Replacement of heat-sensitive elements;
· Repair or replacement of piping;
· Restoration of joint tightness;
· Repair of activation mechanisms;
· Replacement of fasteners;
· Restoration of signal and control lines;
· Recharging or replacement of extinguishing agent cylinders;
All spare parts and materials must: 
· Be new;
· Be unused;
· Comply with the manufacturer’s technical requirements;
· Have supporting quality and fire safety certificates.

	10
	Maintenance
	As part of maintenance, the Contractor shall perform: 
· Cleaning of system components from grease deposits;
· Cleaning of nozzles;
· Checking of cylinder pressure;
· Inspection of piping condition;
· Checking that mountings are in good condition;
· Testing of automatic and manual activation;
· Testing of the interlock system;
· Testing of the system’s interaction with ventilation and process equipment;
· Checking for leaks;
· Testing of the system without discharging the extinguishing agent.

	11
	Requirements for performance of the works 
	The works shall be performed:
· In accordance with applicable fire safety regulations;
· In accordance with the technical documentation of the manufacturer, Brand Kitchen Safe;
· By qualified personnel;
· In compliance with occupational health and safety requirements;
The Contractor shall:
· Ensure the safety of the Customer’s equipment and property;
· Use tools and equipment in good working order;
· Coordinate any equipment shutdown with the Customer’s responsible persons;
· Perform the works with minimal disruption to canteen operations.

	12
	Requirements for the Contractor 
	The Contractor must have: 
· Permits to perform works in the field of fire safety;
· Qualified specialists;
· Experience in performing similar works;
· The necessary clearances and certificates;
· Authorization to service fire suppression systems.

	13
	Testing and commissioning 
	Upon completion of the works, the Contractor shall:
· Test the system’s functionality;
· Test the activation mechanisms;
· Confirm proper interaction with building engineering systems;
· Rectify any identified deficiencies;
· Prepare the system for further operation.
In case of complete equipment replacement: 
· Transportation and delivery of the equipment to the installation site
· Installation of the equipment 
· Commissioning and start-up works
· Staff training 
· Provision of all necessary and relevant equipment documentation (certificates, technical passport, calibration results, etc.)

	14
	As-built documentation 
	Technical passports, certificates of conformity/fire safety certificates, installation and operating instructions, diagrams, declarations, warranty documents.
Design and as-built documentation in electronic (PDF/DWG/DOCX) and hard copy (2 copies).
Certificate of completed works, test reports, settings sheet, as-built diagrams, instructions, logbook.
Commissioning certificate.
Customer staff training record.  


	15
	Quality requirements
	The works shall result in:
· Full restoration of system functionality;
· No faults or leaks;
· Compliance of the system with fire safety requirements;
· Readiness of the system for normal operation.

	16
	Period of performance
	As defined in the contract

	17
	Warranty obligations 
	As defined in the contract

	18
	Special conditions 
	· The works shall be performed at an operating facility in compliance with sanitary and fire safety requirements;
· Damage to existing utility networks is not permitted;
· Upon completion of the works, the Contractor shall clean the work area and remove waste;
· Any changes to the scope of works shall be agreed with the Customer in writing. 

	19
	Payment terms 
	As defined in the contract.
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